BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0169
Directory number subscribed in PSTN?

This command defines if the internal programmed directory number of the extension is in the subscribed PSTN number range. If the directory number is not in the number range, a common number defined by command 1801, is used in case of A- or B- number sending.

##### Valid data

Master only |  | copied to slave: YES / NO |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005