BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2098
Start/Stop indicator for Analogue CLIP

The command is used to define the start and stop value for the analogue CLIP in the analogue interface.

The start indicator is used to inform the analogue phone that DTMF digit sending for analogue CLIP has started.

The stop indicator is used as end point for DTMF digit sending.

Note

The command exists since Release 15 R3A

##### Valid data for start/stop indicator for DTMF sending

no indicator |
DTMF digit A |
DTMF digit B |
DTMF digit C - Initial value - stop indicator |
DTMF digit D - Initial value - start indicator |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005