BusinessPhone Communication Platform 7.0
Dialogs

## CTI

In this dialog, you can define the port number and the individual number of the CTI port. Furthermore, you can set the duration that the PBX will wait for an automatic rerouting position initialized from a CTI telephony server.

To access the dialog, open the “Interfaces” menu in the Configuration directory tree and click on the “CTI” submenu.

The following commands are available:

8901 |  | CTI port

8902 |  | CTI route timeout

For more information about a command or a setting, click on the respective command link in brackets.

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |

See facility description Computer Telephony Integration (CTI) (900/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2005