BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0199
Attenuation for DTMF‑signaling for Analougue CLIP

The command is used to state the attenuation for the DTMF-signaling for analogue CLIP in the analogue interface before it starts ringing.

Note

The command exists since Release 15 R3A

The value of the transmission level is -12.0 dBr to +6.0 dBr in steps of 0.1 dBr.

Initial value = -7.0 dBr.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005