BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1949
Carrier for proprietary services

This command states if UUI (User-to-user Information) is to be embedded in generic functional protocol. When this command is set to ‘embedded’ then commands 1941 Explicit UUS service 1 activation request, 1944 Explicit UUS service 2 activation request and 1945 Explicit UUS service 3 activation request have no function.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005