BusinessPhone Communication Platform 7.0
Installation Instruction ASB 150 02 > Integrated Cordless

## Wireless Relay Station BS370 (KRCNB 303 01/1)

The BS370 Wireless Relay Station (WRS) is a base station without cable connection to the system. The BS370 is connected to a host base station through a radio link. The BS370 provides coverage where cabling is difficult or impossible, e.g. in parking areas.

The radio coverage of the BS370 is comparable to the radio coverage of the BS340.

The BS330, BS340 and DCT1800/Core base station can be used as host base station. All host base stations must have base station software with revision level R2A or higher.

For details refer to Installation instructions BS370 (1531-NTM/KRCNB 303 01 Uen) - available in PDF format on the OaM - CD.

Revision: J © Ericsson Enterprise 2005