BusinessPhone Communication Platform 7.0
Commands > Commands 6000...6999

## 6010
Master/Slave

Determines whether the PABX is 'master' or 'slave' when connected to certain types of local-connected units.

The command determines whether the PABX will be master or slave when connected to an external equipment (V24).

This command will be ignored when connecting certain types of external equipment (see command 6006 Device type).

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

In case of a CTI (with BusinessLink for Windows) connection the command must be set to “1”, meaning that the PABX is used as slave.

Revision: E © Ericsson Enterprise 2005