BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 94 ELDTRANSIT

0A9h ELT_IOSETUP |  | External relay control |
090h ELT_CLEARLED |  | Clear a telephone led |
091h ELT_SETLED |  | Turn on a LED |
0A2h ELT_PESREQ |  | Request from Personal Efficiency System |
0A3h ELT_PESGLOBAL |  | Broadcast info for PES |
0A4h ELT_PESINFO |  | Information for PES |
0A5h ELT_PCOPIREQ |  | Request from PC operator |
0A6h ELT_PCOPIINFO |  | Information for PC operator |

Revision: F © Ericsson Enterprise 2005