BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 4D MICTRL

00h MIMGIND |  | Message indication from MG-block |
01h MIININD |  | Information indication from IN-block |
02h MIHOIND |  | Wake-up indication, DND indication, clear last saved number, individual status for RTR and DID |
03h MIEXIND |  | Voice mail indication from EX-block |
04h MIININDQ |  | Check Voice information from IN-block |
05h MIINREL |  | Release connection and stop play |
06h MIININDANSW |  | Information from IN |
07h MIMGINDQ |  | Check unanswered messages from MG-block |
08h MIMGINDANSW |  | Answer message to MIMGINDQ |
09h MIINDIRECT |  | Direct diversion |
0Ah MIINBUSY |  | Diversion on busy |
0Bh MIINNOREPLY |  | Diversion on no reply |
0Ch MIMGREC |  | Conversation recording indication |
0 MIMGNONE |  | No message to extension |
1 MIMGX |  | Message exists |
2 MIMGCHECK |  | Message checked |
0 MIINNONE |  | No information for extension |
1 MIINTEXT |  | Text information active |
2 MIINVOICE |  | Voice information active |
3 MIINPREDEF |  | Predefined information active |
4 MIINGRTON |  | Ind. mailbox greeting exists |
5 MIINGRTOFF |  | Ind. mailbox greeting does not exist |
0 MIHONONE |  | Wake-up not ordered for extension |
1 MIHOWAKEUP |  | Wake-up ordered for extension |
2 MIHONODND |  | Deactivate Do not disturb for extension |
3 MIHODND |  | Activate do not disturb for extension |
4 MIHOLSCLR |  | Delete last saved number |
5 MIHOINDBARR |  | Individual status for RTR and DID |
0 MIEXNONE |  | No external voice mail to extension |
1 MIEXVMAIL |  | External voice mail to extension exist |
0 MIINNOPLAY |  | No play, if absence information active |
1 MIINPLAY |  | Play voice or predefined info for ext. |
2 MIINRECORD |  | Record personal greeting |
3 MIINERASE |  | Erase personal greeting |
4 MIINSTORE |  | Store personal greeting |
5 MIINREWPLAY |  | Rewind play during configuration of pers.gr. |
4 MIINCONN |  | Connection with IN established |
5 MIINACK |  | Positive answer for PG request |
6 MIINNAK |  | Negative answer for PG request |
7 MIINFAULT |  | Negative answer for PG request |
0 MIINRELNOANSWER |  | No answer message to MG necessary |
1 MIINRELANSWER |  | Answer after VMU channel is released |
0 MIMGRECOFF |  | Conversation recording off |
1 MIMGRECON |  | Conversation recording on |
2 MIMGRECFLASH |  | Conversation recording last 10 seconds |

Revision: F © Ericsson Enterprise 2005