BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0188
Voice transmission quality

This command defines which voice transmission quality table (1-4) shall be used for the call setup to an IP network as well for IP-Extension. Each voice transmission quality table comprises a set of 4 codecs, whereby the access of the codecs relys on a different priority, which will be defined by the following commands:

2165 |  | Voice Transmission Quality Table 1

2166 |  | Voice Transmission Quality Table 2

2167 |  | Voice Transmission Quality Table 3

2168 |  | Voice Transmission Quality Table 4

##### Valid data

1-4 |  | Voice Transmisson Quality table |
3 (default) |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005