BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2143
GK Backup NGK Identifier

For each of the in command 2142 GK Backup NGK RAS transport address specified Backup-NGKs an identifier used for security purpose can be set.

##### Valid data

1-25 |  | 0-16 character |
1-25 |  | empty (default) |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005