BusinessPhone Communication Platform 7.0
Commands > Commands 4000...4999

## 4103
Ringburst at queue

This command is used to state whether a ringing signal (burst) shall be sent to the operator telephone when a queue to busy operator is formed.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005