BusinessPhone Communication Platform 7.0
Commands > Commands 5000...5999

## 5424
Create automated attendant

Via this command is possible to specify the directory numbers of different AA-s (imply: voice menus) you are going to need in your specific application. The first AA (top level) must have a dialable directory number in order that every one uses AA function just by calling it directly. The directory number of all other AA (except the top-level) can (or not) have a non-dialable directory number (e.g. starting with D, *, # etc).

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005