BusinessPhone Communication Platform 7.0
Commands > Commands 3000...3999

## 3704
Queue tone?

This command is used to determine whether callers shall receive queue tone or ringing tone in the queue state if no voice answer is provided. Queue tone is received only if the times in commands 3802 Time for 1st recorded answer and 3803 Time for 2nd recorded answer are set to 0 and the value with this command is Y. If queue tone is supplied, answer signaling to the calling trunk takes place.

Yes = queue tone |  |

No = ringing tone |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005