BusinessPhone Communication Platform 7.0
Dialogs

## Trunk Route Parameters

Facilities of this type can be created/deleted/altered by using the standard facility management dialog. The facility parameters are described below.

Note

You cannot delete trunk route 0, but you can change its directory number and name.

Beside the directory number and name, the following commands are available:

3301 |  | Random Selection

3302 |  | Callback allowed?

3303 |  | Predigits

3304 |  | First alternative route

3305 |  | Predigits for first alternative route

3306 |  | Second alternative route

3307 |  | Predigits for second alternative route

3201 |  | Route members

#### Actions

Submit |  | To send your changes to the system. |
Reload |  | To retrieve the current settings from the system. |
Copy |  | To copy the trunk route settings. |
Back^ |  | To return to the previous window. |

See Facility Descriptions:

- Route Selection (444/15534-ASB 150 02 Uen).
- Trunk (486/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2005