BusinessPhone Communication Platform 7.0
Commands > Commands 7000...7999

## 7446
Heartbeat attempts

This command determines the number of calls that may be made from the heartbeat function in situations where the receiving device does not respond. Value 0-5 .

‘Heartbeat’ means that the PABX makes a call to a specified external number to show that it has not stopped functioning.

Commands 7420 Service area id, 7421 Identity of exchange and 7440 Heartbeat on?-7447 Heartbeat pace concern the heartbeat function.

Note

Value 0 means the string is not send via Modem, but used for direct connections via the CPU- or AUX- port.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2005