BusinessPhone Communication Platform 7.0
Commands > Commands 8000...8999

## 8736
Mobile Access reroute position on no authorization

If an external party (mobile extension) calls a Mobile group (access number) and the received A-number is not assigned to any Mobile Extension directory number (see command 2270 Assign A-number of Mobile Extensions) the call is rerouted to the answering position specified by this directory number.

##### Valid data

Decimal number |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005