BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 61 BTCORDER

01h BTOSEIZURE |  | Seizure trunk for outgoing call |
02h BTODETEPTS |  | Detect 'proceed to send' signal |
03h BTOSTDEPTS |  | Stop detect 'proceed to send' signal |
04h BTOPARKING |  | Put trunk in parking condition |
05h BTOSPEECH |  | Put trunk in speech condition |
06h BTORELEASE |  | Send release to PE |
07h BTOFWEOS |  | Forward EOS (register signalling ready) |
09h BTOINQUIRY |  | Initiate inquiry in PE |
0Ah BTOSEOSFREE |  | Send EOS signal, extension free |
0Bh BTOSEOSBUSY |  | Send EOS signal, extension busy |
0Ch BTOBLOCK |  | Block individual trunk |
0Dh BTODEBLOCK |  | Deblock individual trunk |
0Eh BTOSENDPTS |  | Send 'proceed to send' signal |
0Fh BTOSEOS |  | Send EOS signal |
10h BTOSENDPES |  | Send (periodic) end signal |
11h BTOSENDSEIZ |  | Send seize signal to PE |
12h BTOSENDREL |  | Send release signal to PE |
13h BTODETESPTS |  | Detect special proceed-to-send signal |
20h BTOSEIZACK |  | Seizure accepted |
21h BTOSEIZNAK |  | Seizure rejected |
22h BTOLOOP |  | Loop back line on net side |
23h BTODELOOP |  | Stop loop back line on net side |

Revision: F © Ericsson Enterprise 2005