BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0174
Alarm group

The command is used to assign an extension to an alarm group. Alarm groups are used to join extensions equiped with an external alarm button in order to signal alarms to different alarm centers.

##### Valid data

0 |  | (default) |
1-7 |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005