BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1308
PTS-signal from parent exchange = dial tone?

The command states whether the proceed-to-send signal from the parent exchange is the dial tone.

(Command 1007 Break-in allowed? states whether a proceed-to-send signal is sent by the parent exchange. See also command 1013 Dial tone to extension?, which states whether a dial tone shall be sent to the extension.)

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005