BusinessPhone Communication Platform 7.0
Commands > Commands 6000...6999

## 6804
Internal number length of inband CPN

This command is used to define the maximum number length of the used internal and CN numbers for a given tenant group.

This definition is used to distinguish received inband digits (named inband Called Party Number) either as internal or external numbers and therby followed number analysis.

This command has relevance only when the user category command 0195 CPN modification at call from ME? is activated for handling of public inband CPN’s.

##### Valid data

1-8 |  |  |
4 |  | ldefault for tenant group 0‑15 |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005