BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0x10
System Restart

Default definition: |  | ALARM + NOPROG + EXTERN + ACTIVE |
Used by block: |  | OS, RP |
Category: |  | DESIGNER |

This code is used by OS to report the restart reason.

- D1: Last OS phase before restart. See ‘OSLPHASEOLD’
- D2: Last executed ST before restart. See ‘OSLJOBSTOLD’
- D3: Restart reason

- 00H ... Purpose of restart not specified
- 01H ... FW remote upgrading, set by SU
- 03H ... E2 conversion, set by CE
- 04H ... Warning category STOP, set by OM
- 05H ... Restart with OM Tool, set by OM
- 06H ... Restart with system instrument, set by OM
- 07H ... Error in non-mapped RAM, set by OS
- 08H ... Restart of a single peripheral interface board, set by OM

- D4: Undefined

The restart purpose is not available, when the central software is compiled in Release-mode.

This code is also used by peripheral interface boards to force the shutdown and restart of a single card position after a major internal error has been detected.

- D1 - Last executed process ID

- FFH ... Process ID not known

- D2 - Restart reason, defined by the RTOS on the given peripheral interface board
- D3 - Last executed signal number (high byte)
- D4 - Last executed signal number (low byte)

Revision: K © Ericsson Enterprise 2005