BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1312
MFC signal scheme

The command is used to state the signalling table for MFC (MFE/MFP) register signalling.

0 = Standard R2 |  |

1 = Simplified R2 |  |

2 = Finnish R2 |  |

3 = Norwegian R2 |  |

4 = Mexican R2 |  |

5 = Australien R2 |  |

6 = Belgian simpl.R2 |  |

7 = Malaysia R2 |  |

8 = Brazil R2 |  |

9 = Brazil LME |  |

10 = China R2 |  |

11 = Israel R2 |  |

Value = 00-15

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005