BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2070
Keypad characters

The function of the command is to determine the characters that will be echoed at pressing a key represented in the table.

The table shows the keys that are programmable and the characters that will be echoed when the key is pressed repeatedly.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005