BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1314
Type of dial tone receiver, TRC

The command is used to state the type of dial tone register, TRC, (on RSU) to be used.

The command is used for digital trunks.

00 = Standard TRC |  |

Value = 00-00 (- extended in future) |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005