BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0202
Allocate resources for individual short numbers

This command defines the amount of individual abbreviated numbers which shall be assigned to the extension. Individual abbreviated numbers are assigned in groups of four numbers. Command 0202 can be used to minimize allocated resources in the system for programming available individual short numbers.

##### Valid data

Up to the last programmed key |  | If selected, only the memory blocks from the first up to the memory block required to store the data of the last programmed ind. short no. in the list is reserved - 1 memory block consists of 4 ind. short no. - so if e.g. position A is programmed by BMS, the end user can program (if authorized) up to 4 ind. short no. (depending on the phone type) |
For all provided keys |  | If selected, then all the memory for this type of phone is reserved! The end user can program all ind. short numbers of his phone! |

The value of this command is not stored in the connected BusinessPhone system. The value is sent towards BusinessPhone after submitting this page in order to define the allowed key resources.

Default value is "for all provided keys".

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005