BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2501
Programming of abbreviated numbers

Each common abbreviated number is programmed in an abbreviated number table.

- Enter directory number for abbreviated number
- Enter relevant abbreviated number.
  maximum 23 digits (1-9, 0, *, #).

Default data = No number

Special characters in the number string:

“-” to wait for an intermediate dial tone

In order to wait for an intermediate dial tone include the character “-” in the abbreviated number string

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005