BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## C7 CILCONSTAT

0 CON.REG |  | Register |
1 CON.RING |  | Ringing |
2 CON.SPEECH |  | Speech |
4 CON.TTTB |  | Totally transparent, totally busy |
5 CON.TTNB |  | Totally transparent, normal busy |
6 CON.PTNB |  | Partial transparent, normal busy |
8 CON.OPTEST |  | Test of operator instrument |
9 CON.VPAG |  | Group voice paging |
10 CON.WAIT |  | Waiting, queued |
11 CON.BREAKA |  | Break-in 'A'-part |
12 CON.BREAKB |  | Break-in 'B'-part |
13 CON.BREAKC |  | Break-in 'C'-part |
14 CON.CONF |  | Conference |
15 CON.TTTBV |  | Totally transparent, totally busy, volume |
16 CON.TTNBV |  | Totally transparent, normal busy, volume |
17 CON.PTNBV |  | Partial transparent, normal busy, volume |
18 CON.REGREQ |  | Register, request of keys one by one |
19 CON.ALERT |  | Ringing started in network |
20 CON.PROCEED |  | End of selection in network |
21 CON.SPEECHREG |  | Speech and register state |
22 CON.PROGRESS |  | Progress indicator from ISDN line |
23 CON.CONREC |  | Conversation recording facility |
24 CON.3PTYCONF |  | External Call Hold and External Conference facility |

Revision: F © Ericsson Enterprise 2005