BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## CB EUCTRL

00h EUCSZACK |  | Seizure (EUSEIZ) acknowledge |
01h EUCSZNAK |  | Seizure (EUSEIZ) negative acknowledge |
02h EUCCALL |  | Call from connected PC/terminal |
03h EUCONRDY |  | Ready for transfer |
04h EUCONREL |  | Release IO-connection |
05h EUCONEND |  | IO-connection released |
06h EUCMCALLOW |  | Allow multiplexed communication |
07h EUCWAITREQ |  | Request to interrupt current output |
08h EUCWAITACK |  | Interrupt acknowledged |
09h EUCWAITNAK |  | Interrupt not acknowledged |
0Ah EUCWAITRDY |  | Current output is completed, ready to wait |
0Bh EUCRESUME |  | Resume interrupted output |
0Ch EUCBUSY |  | ASB-block is busy, answer to EUCCALL |
0Dh EUCRDYSWUPD |  | Ready for remote software update |

Revision: F © Ericsson Enterprise 2005