BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0x74
No Default E2Data Reported.

Default definition: |  | ALARM + NOPROG + EXTERN + ACTIVE |
Used by block: |  | SU |
Category: |  | MAINTENANCE |

SU did not find default data, corresponding to this individual type. Some card handling CP program is possibly missing.

- D1: Card position
- D2: Version/type of individual from the CARDREP message
- D3: Undefined
- D4: Undefined

#### Recommended action

Verify that the software on the CPU-board has the correct version.

Revision: K © Ericsson Enterprise 2005