BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0196
Line Attenuation Rating

This command defines the attenuation value, which shall be used between an analogue trunk and a DBC 222.

Note

The command exists since Release 15 R2A

##### Valid data

Value | Attenuation
0 | 0 dB
3 | - 3 dB
6 | - 6 dB
9 | - 9 dB
12 | - 12 dB
15 | not programmed (default)

Note

The value is needed for script programming

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005