BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2030
Disconnection tone for digital extensions

If the other party goes on-hook, an analogue extension always receives a disconnection tone (max 8 sec), for a digital extension (with L1,L2 and Inquiry) the disconnection tone is optional.

No: Extension disconnected directly without any tone. |  |

Yes: Extension disconnected with tone (max 8 sec). |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005