BusinessPhone – Dialog 4223 Professional / Dialog 3213
BEA Dialog Description

## DSS connected

The Key panel dialog shows an interactive illustration of the DSS unit(s). DSS stands for Direct Station Select, another name for the optional key panel that is connected to your system telephone.

A red lamp indicates that a function or an Individual Abbreviated Number (or both) has been assigned to the key. Move the mouse over the programmable keys of the DSS unit to view the key parameters key name, key function, assigned number/id, and individual short number.

Additional, a green spot appears on the selected key. Click on the selected key to close the pop-up window and to bring up the Key parameters dialog. In this dialog, you can change the key function, the assigned number or id, and select a ring alternative and a priority, if available. See also Key Parameters.

Now change the key parameters as desired. If you are satisfied with your changes, click on submit in the control bar below to save your changes within the system.

#### Actions

reload |  | To retrieve a programmed number from the system. |
previous |  | To view the programming of the previous key. |
next |  | To view the programming of the following key. |
close |  | To close the Key panel dialog. |

© Ericsson Enterprise 2003