BusinessPhone – Dialog 4224 Operator / Dialog 3214
ISDN Facilities

## Number Identification

The main difference compared to the analog public net is the Number Identification between the connected parties.

When you establish an outgoing external call, the public number of your system and your extension number will be sent to the called party. If the number of the answering party is different from the dialled one (for example, after a diversion), you will also be informed about the answering party’s number.

When you answer an incoming external call on your phone (or from another phone), you will see the caller’s number on the display. Your public number will be sent to the caller.

© Ericsson Enterprise 2003