BusinessPhone – Dialog 4224 Operator / Dialog 3214
Attendance

## Night Switch

This function switches the whole system to the Night Switch mode. The Night Switch mode routes all incoming external calls to a defined night answering position e.g. an answering machine.

Night

Press to activate (pre-programmed)

The lamp lights. Night Switch active.

Night

Press again to deactivate (pre-programmed).

The light extinguishes. Night Switch passive.

© Ericsson Enterprise 2003