BusinessPhone – Dialog 4224 Operator / Dialog 3214
Call Metering

## Operator supervised call

An extension can order an external call to be metered. The caller can remain on the line or hang up (off line) while you establish the call.

#### Option 1

Registration on the callers individual call meter:

Set up the external line.

See section Make external calls.

External dial tone.

Press (see display).

Continue setting up the external call, see section Call Ordering.

Recall after the call is terminated:

Press.

The display informs about call duration, number of pulses or cost (depending on the configuration). Note the information.

If you want to register the cost information:

Press again.

The call is registered on the callers individual call meter.

Clear

Press to disconnect the call.

#### Option 2

Registration on a specified Account Number:

Account

Press (pre-programmed).

Dial the Account Number.

Account

Press again (pre-programmed).

Continue setting up the external call.

© Ericsson Enterprise 2003