BusinessPhone – Dialog 4224 Operator / Dialog 3214
Outgoing Calls

## Busy external line

If no external line is available for your call:

Notify

Press.

Loop 1

Press any free Loop key.

The key lamp shows steady light. You can answer new incoming calls.

A ringing signal and the Loop key lamp flashing indicates that an external line is available.

Loop 1

Press again.

The Loop key light extinguishes. External dial tone. Continue making the external call.

#### Intrusion on a busy external line

You can break into a busy external line.

Press and hold (see display).

The conversation partner of the busy external line, is shown in the display.

Speech

Press to intrude.

A warning tone is heard. Inform the external line of the new call.

Speech

Press again.

The person talking on the external line is disconnected.

© Ericsson Enterprise 2003