BusinessPhone – Dialog 4224 Operator / Dialog 3214
During Calls

## Operator hold

Several incoming calls can be put on hold using this function.

You have speech connection with the caller.

Hold

Press (pre-programmed).

The call is put on hold. The key lamp shows a steady light. You can answer new incoming calls and also put calls on hold by pressing the key again during an ongoing call.

When you want to retake one of the calls on hold, you must be free from ongoing calls:

Hold

Press (pre-programmed).

The oldest call on hold is shown in the display.

Speech

Press to retake.

The call is retaken. The Hold key lamp remains lit if more calls are still on hold.

Or:

Hold

Press (pre-programmed).

The call is put on hold again. The next call on hold is shown.

Repeat until the required call is shown.

When all calls are retaken the key lamp extinguishes.

© Ericsson Enterprise 2003