# Logical Switch

1. SAN A
   1 networks
   2 ports
2. Corporate
   3 networks
   2 ports
3. SAN B
   1 networks
   2 ports

1. 1. enc-001, switch 1
      1. warning
         X1
         7 GB/s
         ok
         X1
         7 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      2. ok
         X2
         2 GB/s
         ok
         X2
         2 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      3. disabled
         X3
         0 GB/s
         disabled
         X3
         0 GB/s
         00:17:A4:77:C0:70
      4. error
         X4
         0 GB/s
         error
         X4
         0 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      5. warning
         X5
         8 GB/s
         ok
         X5
         8 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      6. ok
         X6
         2 GB/s
         ok
         X6
         2 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      7. ok
         X7
         1 GB/s
         ok
         X7
         1 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      8. ok
         X8
         1 GB/s
         ok
         X8
         1 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
   2. HP Virtual Connect Flex-10 10Gb Ethernet Module
      1. warning
         X1
         7 GB/s
         ok
         X1
         7 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      2. ok
         X2
         2 GB/s
         ok
         X2
         2 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      3. disabled
         X3
         0 GB/s
         disabled
         X3
         0 GB/s
         00:17:A4:77:C0:70
      4. error
         X4
         0 GB/s
         error
         X4
         0 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      5. warning
         X5
         8 GB/s
         ok
         X5
         8 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      6. ok
         X6
         2 GB/s
         ok
         X6
         2 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      7. ok
         X7
         1 GB/s
         ok
         X7
         1 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      8. ok
         X8
         1 GB/s
         ok
         X8
         1 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
2. 1. enc-001, switch 3
      1. warning
         X1
         7 GB/s
         ok
         X1
         7 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      2. ok
         X2
         2 GB/s
         ok
         X2
         2 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      3. disabled
         X3
         0 GB/s
         disabled
         X3
         0 GB/s
         00:17:A4:77:C0:70
      4. error
         X4
         0 GB/s
         error
         X4
         0 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      5. warning
         X5
         8 GB/s
         ok
         X5
         8 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      6. ok
         X6
         2 GB/s
         ok
         X6
         2 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      7. ok
         X7
         1 GB/s
         ok
         X7
         1 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      8. ok
         X8
         1 GB/s
         ok
         X8
         1 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
   2. enc-001, switch 4
      1. warning
         X1
         7 GB/s
         ok
         X1
         7 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      2. ok
         X2
         2 GB/s
         ok
         X2
         2 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      3. disabled
         X3
         0 GB/s
         disabled
         X3
         0 GB/s
         00:17:A4:77:C0:70
      4. error
         X4
         0 GB/s
         error
         X4
         0 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      5. warning
         X5
         8 GB/s
         ok
         X5
         8 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      6. ok
         X6
         2 GB/s
         ok
         X6
         2 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      7. ok
         X7
         1 GB/s
         ok
         X7
         1 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      8. ok
         X8
         1 GB/s
         ok
         X8
         1 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
3. 1. enc-001, switch 5
      1. warning
         X1
         7 GB/s
         ok
         X1
         7 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      2. ok
         X2
         2 GB/s
         ok
         X2
         2 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      3. disabled
         X3
         0 GB/s
         disabled
         X3
         0 GB/s
         00:17:A4:77:C0:70
      4. error
         X4
         0 GB/s
         error
         X4
         0 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      5. warning
         X5
         8 GB/s
         ok
         X5
         8 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      6. ok
         X6
         2 GB/s
         ok
         X6
         2 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      7. ok
         X7
         1 GB/s
         ok
         X7
         1 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      8. ok
         X8
         1 GB/s
         ok
         X8
         1 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
   2. enc-001, switch 6
      1. warning
         X1
         7 GB/s
         ok
         X1
         7 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      2. ok
         X2
         2 GB/s
         ok
         X2
         2 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      3. disabled
         X3
         0 GB/s
         disabled
         X3
         0 GB/s
         00:17:A4:77:C0:70
      4. error
         X4
         0 GB/s
         error
         X4
         0 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      5. warning
         X5
         8 GB/s
         ok
         X5
         8 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      6. ok
         X6
         2 GB/s
         ok
         X6
         2 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      7. ok
         X7
         1 GB/s
         ok
         X7
         1 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1
      8. ok
         X8
         1 GB/s
         ok
         X8
         1 GB/s
         00:17:A4:77:C0:70
         uplink group 1
         network 1