#

10. Snmp

1. ## Errors

   1. Appliance host name
      Changing the hostname requires generating a new SSL certificate for secure communications with your browser.
2. 1. Address Assignment
      DHCP is not recommended for assigning appliance IP addresses unless DHCP reservations are used
   2. DHCP configuration is not allowed
   3. IP Adress
      from DHCP Changing the IP address requires generating a new SSL certificate for secure communications with your browser.
   4. Second IP Address
   5. Subnet mask or CIDR
      from DHCP
   6. Gateway address
      from DHCP Specify gateway address if the appliance needs to be accessed from a different subnet
3. 1. Preferred DNS server
      from DHCP
   2. Alternate DNS server
      from DHCP
4. 1. Address Assignment
      Unassign DHCP is not recommended for assigning appliance IP addresses unless DHCP reservations are used When the appliance is configured for IPV6 access, ensure that the DNS servers configured in your appliance network has support for both IPV4 and IPV6 name resolution. DHCP configuration is not allowed
   2. IP Address
      from DHCP
   3. Subnet mask or CIDR
      from DHCP
   4. Gateway address
      from DHCP Specify gateway address if the appliance needs to be accessed from a different subnet

5. 1. |  | Usage | Hostname | IP Address | MAC Address |  |

6. Services
7. Web Server

   1. ## Warning

   2. certificate
      Private Key
8. certificates

   ## Errors

   1. ## Warning

   2. Import RabbitMQ
      Server certificate
      CA certificate
      Private Key
   1. Import RabbitMQ
      Server certificate
      CA certificate
      Private Key

9. ## Errors

   1. Manual Synchronize with time server
   2. Network time servers
   3. Recommended
   4. Recommended
   5. Current date and time
   6. Current date and time
      Changing the current date and time of the appliance will affect all the logged-in users and current jobs that are running in the appliance, so a reboot of the appliance is mandatory after applying the change.
      The appliance will reboot on manual date time setting.
   7. Locale
      Locale changes will be reflected only after rebooting the appliance.
10. SNMP
    1. Read community string

    2. Trap Destination | Port | Community String |  |

    3. Add trap destination

Applying network settings...

Accept certificates when the browser prompts you to.

Loading ...