1. [General]
   1. [Description]
      [MS Exchange 2010 Gold, 5000 Users]
   2. [Server type]
      [Proliant BL460c G7, mezz1]
   3. [Firmware baseline]
2. [Connections]

   [TBD]

3. [BIOS]

   ### [Managed by Fusion]

   - [Modified]
   - [All]
   [System options]
   [Advanced Memory Protection] | [Online Spare with Advanced ECC Support]
   [NUMLOCK Power-On State] | [Default On]
   [Processor Options] [System Options]
   [No-Execute Memory Protection] | [Default] [Optimized for Performance]
   [Intel/AMD Virtualization Technology] | [Default] [Enabled]
   [Intel Hyperthreading Options] | [Disabled]
   [Intel Turbo Boost Technology] | [Optimized for Low Power]
   [Intel VT-d/AMD-Vi (IOMMU)] | [Default Enabled]
   [SATA Controller Options] [System Options]
   [Embedded SATA Configuration] | [Default] [Enabled]
   [Device Write Cache] | Default [Enabled]
   [Serial Port Options] [System Options]
   [Embedded Serial Port] | [Default] [COM 2; IRQ3; IO: 2F8h-2FFh]
   [Virtual Serial Port] | [Default][COM 1; IRQ4; IO: 3F8h-3FFh]