# [Find Node Range]

1. [Enter IP Address]
   [Choose type of search to use to find nodes]
2. [Enter IP Address]
   [Start IP Address]
   [End IP Address]
   [Port to Scan]
   [Invalid IP Address or Range specified]
3. [Enter LDAP Server Address]
   [LDAP Server]
   [Username]
   [Password]
   [Max Return]
   [Invalid LDAP Server or Username or Password specified]
4. [Search in Progress]
5. [Available Nodes]

   [IP Address] | [DNS Target Name]

7. [Added Nodes]

   [IP Address] | [DNS Target Name]

# [Add Nodes]

1. [General]
2. 1. [Prerequisites installation option]
   2. [Install iLO Channel Interface Driver if not already installed]
      [Warning: if CHIF driver is not already installed, inventory an recomemnded updates may be incomplete on Gen9 and older generation servers. Gen10 servers require CHIF driver to be installed]
3. [Baseline to Apply]
   [Optional. Select an already added and inventoried baseline and/or additional package to apply to this node. If not added now, a baseline or additional package must be specified when Inventory is started on the node.]

   1. [Baseline]
   2. [Additional Packages]
4. [Credentials]
   1. [Use Current Credentials (requires existing trust relationship with the target)]
   2. [Enter Administrator Credentials]
   3. [Enter SSH key credentials]
   1. [Username] [Required]
   2. [Password] [Required]
   1. [Username] [Required]
   2. [Required]
   3. [Passphrase]
   4. [Required only if a passphrase is required for the private key file]
5. [iLO Credentials]
   [iLO credentials are required in addition to host OS credentials when the iLO for a server is configured in one of the high security modes. The account provided must have ‘Configure iLO Settings’ permissions in order to perform firmware updates.] [Note: Only applies to systems with iLO.]
   1. [Username]
   2. [Password]