1. [General]
   1. [Model]
      HP VC Flex-10 Enet Module
   2. [Serial number]
      TW0000001F
   3. [Firmware version]
      8.0.2009-10-07T10:16:12Z
   4. [Location]
      Atlanta / rack 12 / enc-001.my.com
   5. [Devices]
2. [Connectivity]

   ### [Uplinks]

   1. | [Port] | [Type] | [Address] | [Speed] | [Utilization] | [Networks]
      ok | X1 | Ethernet | 00:17:A4:77:C0:70 | 4 Gb/s |  | 2 networks
      [Connector]
      [Identifier] | [Extended] | [Bandwidth] | [Vendor] | [OUI] | [Part number] | [Revision]
      SFP | 0x04 | 10 Gb/s | Avago | 0x00176a | ABCU-1234-X |
      [Remote connection]
      [Type] | [Discovered time] | [Port type] | [Port ID] | [Port description] | [Address type] | [Address]
      External | 123456789 | Local | 12 | 12 | IPv4 | 16.125.28.2
      [System name] ProCurve 2910 Switch 25-12 [System description] ProCurve 2910 Switch 25-12 [Statistics] [Transmitted errors] 2 [Received errors] 0 [Bit Transfer Rate] [Packet Transfer Rate]
      ok | X2 | Ethernet | 00:17:A4:77:C0:71 | 4 Gb/s |  | 3 networks
      [Connector]
      [Identifier] | [Extended] | [Bandwidth] | [Vendor] | [OUI] | [Part number] | [Revision]
      SFP | 0x04 | 10 Gb/s | Avago | 0x00176a | ABCU-1234-X |
      [Remote connection]
      [Type] | [Discovered time] | [Port type] | [Port ID] | [Port description] | [Address type] | [Address]
      External | 123456789 | Local | 12 | 12 | IPv4 | 16.125.28.2
      [System name] ProCurve 2910 Switch 25-12 [System description] ProCurve 2910 Switch 25-12 [Statistics] [Transmitted errors] 2 [Received errors] 0 [Bit Transfer Rate] [Packet Transfer Rate]

   ### [Downlinks]

   1. | [Port] | [State] | [Server hardware] | [Adapter port] | [Server profile] | [Utilization]
      ok | Port 1 | Enabled | enc-001, bay 1 | LOM 1 | server 1 |
      |  | [Flex NIC] | [Link state] | [Type] | [Address] | [Network(s)] | [Bandwidth Gb/s] | [Utilization]
      | ok | LOM 1-a | Linked | Ethernet | 00:17:A4:77:C0:70 | network 1 | 3.4 / 8.0 |
      [Connection state] Active [Transmit errors] 2 [Bit Transfer Rate] [Packet Transfer Rate]
      | warning | LOM 1-b | Unlinked | Fibre Channel | 00:17:A4:77:C0:72 | SAN A | 3.4 / 8.0 |
      TBD
      | ok | LOM 1-c | Linked | Ethernet | 00:17:A4:77:C0:74 | network 2 | 3.4 / 8.0 |
      TBD
      ok | Port 2 | Enabled | enc-001, bay 2 | LOM 1 | server 2 |