 	 
inventory
Enables you to scan nodes for the currently installed version of firmware, drivers, and hardware components.

Syntax

smartupdate inventory [--nodes <nodelist>] [--baselines <baselinelist>]

Parameters

--nodes [<nodelist>]
A list of the nodes on which to perform the inventory command. You can specify each node in the following ways:

localhost
127.0.0.1
::1
--baselines [<baselinelist or install_set_name>]
Specify the path of the SPP or components. If the baseline location includes spaces or special characters, use escape characters (Linux) or double-quotations (Windows).

To use a saved install set on the iLO Repository, include a node IP address or DNS name and the baseline install set name.

If you include a node list with the baseline, SUM performs inventory on the nodes with the baseline specified. If you do not include a node list, then SUM only performs inventory on the baseline.

Restrictions

Set the management options (use_ams, use_wmi, use_snmp, no_mgmt) with the setattributes parameter before performing inventory.

After performing successful inventory on a VC node using an encryption key, use the setattributes command to assign the encryption_key parameter details.

Windows usage

C:\>smartupdate inventory /nodes 10.0.1.1 /baselines C:\Users\Administrator\Desktop\blds\ilo\26.33

C:\>smartupdate inventory /nodes 10.0.1.1 /baseline <install_set_name>

Linux usage

$ ./smartupdate inventory --nodes 10.0.1.1 --baselines /root/Desktop/rono/blds/ilo

Return codes
SUCCESS_NO_REBOOT
Windows: 0

Linux: 0

Text: The command was successful.

SUCCESS_REBOOT
Windows: 1

Linux: 1

Text: The command was successful but a reboot is required.

SUCCESS_NOT_REQUIRED
Windows: 3

Linux: 3

Text: The command completed successfully, but was not required or everything is already current.

FAILURE_GENERAL
Windows: -1

Linux: 255

Text: A general failure occurred. For details, see the logs.

FAILURE_BAD_PARM
Windows: -2

Linux: 254

Text: A bad input parameter was encountered. For details, see the logs.

FAILURE_COMPONENT_FAILED
Windows: -3

Linux: 253

Text: The installation of the component failed.

FAILURE_COMMAND_FAILED
Windows: -4

Linux: 252

Text: The command failed. For details, see the logs.

 	 	 