# [Deploy]

2. [Baseline to Apply]
   1. 1. [Node needs to be removed]

      2. [Remove node from the group]

      3. [Select an already added and inventoried baseline and/or additional package to apply to this node.]

      4. [Baselines]
      5. [Additional Package]
3. [nodeName] [nodeName]
   [nodeType] [nodeType]

   [nodeType] | [nodeType] [nodeType]

   2. [estimated deploy time]

   2. [Number of components] |
      [Number of components] |
      [Number of components] |
      [SUM updatable components] |
      [UEFI updatable components] |
      [iLO updatable components] |

4. 1. 1. 1. 1. [Options]
         2. [Enable verbose logging from components]
         3. [Skip components with dependency failures]
         4. [Ignore Warnings]
         5. [Clean up temporary files after deploy]
         6. [Clean up all debug logs and temporary files after deploy]
      2. [Encryption Settings]
         [Encryption Key]
         [VC Domain is in FIPS mode. Encryption Key is mandatory. Requires minimum 8 characters]
      3. [Activation Order]
         [VC Enet Modules Activation Order]
         [VC FC Modules Activation Order]
         [Activation Delay]
         [VC Enet Modules Activation Delay]
         [VC FC Modules Activation Delay]
      4. 1. [Reboot System after installation]
         2. [Reboot Delay (Seconds): ]
         3. [Enter reboot message] [Reboot at user request after deploy]
         4. [Message upto 255 characters]
      5. 1. [Save Install Sets]
         1. [Update Recovery Set]

         ### [iLO Credentials]

         [Note: iLO domain credentials cannot be used to update an iLO Recovery Install Set.]

         [Username] |  | [Required]
         [Password] |  | [Required]

         [availableIloSpace] | [N/A]
         [Name:] |  | [Required]
         [Desription:] |  | [Required]

         ### [iLO Repository Options]

         [Allow SUM to manage iLO Repository space] [Manually manage iLO Repository space]
         [Delete existing Install Set]

      6. 1. [Reboot node to activate firmware]
         2. [Reboot is not required. The node is powered off]
      7. 1. [Exclude nPar Firmware]
      8. 1. [Reboot nPar(s) to activate firmware]
         2. [Reboot is not required, nPar(s) are powered off]
5. 2. 1. 1. [Rewrite is not supported for VMWare drivers]
            [FIPS mode is ON. Downgrade/Re-write of OA firmware is not allowed.]
      2. [FIPS mode is ON. Downgrade/Re-write of OA firmware is not allowed.]

         1. | [Deploy Enclosure]

# [Applicable Components]

[Applying installation options. Please wait...]

[Applicable components are re-populated after analysis.]

[Pausing schedule temporarily.]