# [Add Node]

1. [Nodes]
   1. [Select operation]
   3. [IP/DNS]
   4. [Description]
   5. [Node type]
      [Automatically Add Associated Nodes]
2. 1. [If active update process is detected on the remote node, SUM should]
   2. [Leave the update running and bypass the node]
   3. [Stop any currently running update process on the node and replace it with updates from this session]
3. 1. [Prerequisites installation option]
   2. [Install iLO Channel Interface Driver if not already installed]
      [if CHIF driver is not already installed, inventory and recommended updates may be incomplete on Gen9 and older generation servers. Gen10 and above servers require CHIF driver to be installed]
4. [Baseline to Apply]
   [Optional. Select an already added and inventoried baseline and/or additional package to apply to this node. If not added now, a baseline or additional package must be specified when Inventory is started on the node.]

   1. [Baseline]
   2. [Additional Packages]
5. [Group]
   [Group Description]

   1. [Assign to]
6. [Credentials]
   1. [Use Current Credentials (requires existing trust relationship with the target)]
   2. [Enter Administrator Credentials] [Note: iLO domain credentials cannot be used to update an iLO Recovery Install Set.]
   3. [Enter SSH key credentials]
   1. [Username] [Required]
   2. [Password] [Required]
   1. [Username] [Required]
   2. [Required]
   3. [Passphrase]
   4. [Required only if a passphrase is required for the private key file]
   1. [enter Vcenter Administrator Credentials]
   1. [IP/DNS] [Required]
   2. [Username] [Required]
   3. [Password] [Required]
7. [Access Level]
   1. [None]
   2. [Use sudo with credentials entered above]
   3. [Enter Root user credentials to update components]
   1. [Username] [Required]
   2. [Password] [Required]
8. [iLO Credentials]
   [iLO credentials are required in addition to host OS credentials when the iLO for a server is configured in one of the high security modes. The account provided must have Ã¢â‚¬ËœConfigure iLO SettingsÃ¢â‚¬â„¢ permissions in order to perform firmware updates and 'Recovery Set' permissions in order to change iLO recovery set. ] [Note: Only applies to systems with iLO. iLO domain credentials cannot be used to update an iLO Recovery Install Set.]

   1. [Username]
   2. [Password]
9. 2. [Use Credentials Above]
   3. [Enter Administrator Credentials]
      1. [Username] [Required]
      2. [Password] [Required]
10. [Credentials]
    [iLO CM Administrator Credentials]

    1. [Username] [Required]
    2. [Password] [Required]
    [Enter switch credentials (Required only if switch firmware is to be updated)]
    [Switch Credentials]

    [Credentials are not set for the switch]
    [Password Authentication(Applies to XGc only)]
    [Full Authentication]
    1. [Username]
       [Required] [Username not required]
    2. [Password]
       [Password not required]
    3. [Enable Password]
       [Enable Password not required]
    4. [Credentials are the same on both switches]

    [Switch B Credentials]

    [Credentials are not set for the switch B]
    [Password Authentication(Applies to XGc only)]
    [Full Authentication]
    1. [Username]
       [Required] [Username not required]
    2. [Password]
       [Password not required]
    3. [Enable Password]
       [Enable Password not required]
11. HPE Privacy Policy

[Search is in progress. Please wait...]

[Nodes will be populated after search.]