# [Edit]

1. [General]
   1. [IP/DNS]
   2. [Description]
   3. [Type]
      [Automatically Add Associated Nodes]
2. [If active update process is detected on the remote node, HPSUM should]

   1. [Leave the update running and bypass the node]
   2. [Stop any currently running update process on the node and replace it with updates from this session]
3. [Prerequisites installation option]
   1. [Install iLO Channel Interface Driver if not already installed]
      [Warning: if CHIF driver is not already installed, inventory an recomemnded updates may be incomplete on Gen9 and older generation servers. Gen10 servers require CHIF driver to be installed]
4. [Baseline to Apply]
   1. [Node needs to be removed]

   2. [Remove node from the group]
   3. [Optional. Select an already added and inventoried baseline and/or additional package to apply to this node. If not added now, a baseline or additional package must be specified when Inventory is started on the node.]

   1. [Current Baseline selected]
   2. [Baseline]
   3. [Additional Package selected]
   4. [Additional Packages]
5. [Credentials]
   [Note: iLO domain credentials cannot be used to update an iLO Recovery Install Set.]
   1. [Enter Administrator Credentials]
   2. [Enter SSH key credentials]
   1. [Username]
   2. [Password]
   1. [Username] [Required]
   2. [Required]
   3. [Passphrase]
   4. [Required only if a passphrase is required for the private key file]
   [iLO CM Administrator Credentials]

   1. [Username]
   2. [Password]
   [Switch Credentials]

   [Credentials are not set for the switch]
   [Password Authentication(Applies to XGc only)]
   [Full Authentication]
   1. [Username]
      [Required] [Username not required]
   2. [Password]
      [Password not required]
   3. [Enable Password]
      [Enable Password not required]
   1. [Credentials are the same on both switches]

   [Switch B Credentials]

   [Credentials are not set for the switch B]
   [Password Authentication(Applies to XGc only)]
   [Full Authentication]
   1. [Username]
      [Required] [Username not required]
   2. [Password]
      [Password not required]
   3. [Enable Password]
      [Enable Password not required]
6. [VCenterCredentials]
   1. [Use VCenter]
   1. [IP/DNS] [Required]
   2. [Username] [Required]
   3. [Password] [Required]
7. [Access Level]
   1. [None]
   2. [Use sudo with credentials entered above]
   3. [Enter Root user credentials to update components]
   1. [Username]
   2. [Password]
8. 2. [Use Credentials Above]
   3. [Enter Administrator Credentials]
   1. [Username]
   2. [Password]
9. [Virtual Connect Options]
   [VC Activation options]
   [Activation Order]
   1. [VC Enet Modules Activation Order]
   2. [VC FC Modules Activation Order]
   [Activation Delay]
   1. [VC Enet Modules Activation Delay]
   2. [VC FC Modules Activation Delay]
10. [iLO Credentials]
    [iLO credentials are required in addition to host OS credentials when the iLO for a server is configured in one of the high security modes. The account provided must have ‘Configure iLO Settings’ permissions in order to perform firmware updates.] [Note: Only applies to systems with iLO. iLO domain credentials cannot be used to update an iLO Recovery Install Set.]
    1. [Username]
    2. [Password]
11. HPE Privacy Policy