==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.15.06
==========================================================================
Version: 3.15.06
Release Date: 2021.09.09
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.15.06_rom.ima with checksum          : 1963A218
2. s5xhv3.15.06_rom.ima with MD5 checksum      : 04b758b929a7ebc08f9ebb2ec552b2ae
3. s5xhv3.15.06_rom.ima_enc with MD5 checksum  : 490eebe6a5399d929137cc87e22e2b6c

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R06_20210122 )
SKU 1~2	: R05 (S5X_2.5_R06_20210122 )
S5XQ:
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
S5XH/S5XQH:
1. [CS-BMC] WEB UI UpdateService change the default settings from overwrite to preserved.
2. [CS-BMC] WEB UI Power Control String modify.("ACPI Shutdown" to "Orderly Shutdown")
3. [CS-BMC] Disable IPMI 1.5 and Enable IPMI 2.0 only.(Please remember to add "-I lanplus" parameter in the IPMI command.)
4. [BMC] Define Intel OCP card Device Name in the table.

[Bug Fixed]:
S5XH/S5XQH:
1. [BMC] Fix the controller_name on WebUI RAID Controller Information page to prevent showing the extra space.
2. [BMC] Fix SNMPv3 ask BPS DIMM will not get the correct Memorydevice info.
3. [BMC] Fix Temp_CPU0/1 sensor threshold is not sync between sensor list and sdr list full -v.
4. [Redfish] Fix Redfish password will not restore to default when BMC restore to default.
5. [Restful] Fix RESTful API Error Code 1453 response is inconsistent when set invalid password.

[Known Issues]:
S5XH/S5XQH:
1. [Redfish] Hitachi requirements is not ready.(Virtual Drive Information)
2. [Redfish] Will get "Unkown" Sensor type via Redfish Logs.
3. [BMC] BMC sometimes will logged "Unknown | sensor of type Unknown | (Unknown OEM D0 SEL)" SEL Log event.

[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to ~3.15.06, please use SOCFlash.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.14.06
==========================================================================
Version: 3.14.06
Release Date: 2021.07.23
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.14.06_rom.ima with checksum          : 196438E6
2. s5xhv3.14.06_rom.ima with MD5 checksum      : c4168f3d0a45f473a50b379493adb29c
3. s5xhv3.14.06_rom.ima_enc with MD5 checksum  : dae4f90c58aa32b083795362e1b03a4c

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R06_20210122 )
SKU 1~2	: R05 (S5X_2.5_R06_20210122 )
S5XQ:
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
N/A

[Bug Fixed]:
S5XH/S5XQH:
1. [Redfish] Fix Redfish not ready issue.
2. [BMC] When user Local time zone is GMT -X will cause BMC Event Log keep processing.
3. [BMC] WEB UI System Inventory will not show full information.
4. [BMC] WEB UI Settings --> NIC Management will not show NIC Cards Informations.
5. [BMC] Use Yafuflash to update BIOS with preserve script will not preserve BIOS settings.

[Known Issues]:
1. [Redfish] Hitachi requirements is not ready.(Virtual Drive Information)
2. [Redfish] Will get "Unkown" Sensor type via Redfish Logs.
3. [Redfish] Insert Intel NIC Card will let WEB UI System Inventory to need more time to get information. 
4. [BMC] BMC sometimes will logged "Unknown | sensor of type Unknown | (Unknown OEM D0 SEL)" SEL Log event.

[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to 3.12.06, please use SOCFlash.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.13.06
==========================================================================
Version: 3.13.06
Release Date: 2021.06.17
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.13.06_rom.ima with checksum          : 1962C3E3
2. s5xhv3.13.06_rom.ima with MD5 checksum      : e54375cd403002d20cfe741cb07bb2ba
3. s5xhv3.13.06_rom.ima_enc with MD5 checksum  : 0601213a2963c0853a9a563c43642006

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R06_20210122 )
SKU 1~2	: R05 (S5X_2.5_R06_20210122 )
S5XQ:
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
N/A

[Bug Fixed]:
S5XH/S5XQH:
1. [BMC] Fix caterr issue.
2. [BMC] Fix conf protect while AC lost.
3. [BMC] Fix Nvme rear temp.
4. [BMC] Fix fan reading overflow.
5. [BMC] Fix AC lost event.
6. [BMC] Fix yafuflash update bmc.

[Known issue]:
1. [Redfish] Hitachi requirements is not ready.(Virtual Drive Information)

[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to 3.12.06, please follow below method:
	Method 1: follow below step:
	Step1: ipmitool raw 0x32 0x8f 0x01 0x02  
	Step2: ipmitool mc reset cold  
	Step2-1: Wait BMC Ready	
	Step3: ipmitool raw 0x32 0x8f 0x01 0x04  
	Step4: update 3.05 via webui or yafuflash
	If both fail, please use socflash for 3.05.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.12.06
==========================================================================
Version: 3.12.06
Release Date: 2021.05.28
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.12.06_rom.ima with checksum          : 19B2C7F2
2. s5xhv3.12.06_rom.ima with MD5 checksum      : b0bebd631c1128169b93cbd0579c78d4
3. s5xhv3.12.06_rom.ima_enc with MD5 checksum  : 3c224ae3079cf9bcf592db61f182f97f

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R06_20210122 )
SKU 1~2	: R05 (S5X_2.5_R06_20210122 )
S5XQ:
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
S5XQH:
1. [BMC] Add Fan STB on event by OCP.  

[Bug Fixed]:
N/A

[Known issue]:
1. [BMC] For S5XH, PSU LED and BP LED will be LID if insert Intel OCP 3.0 Card even is Power Off.
2. [BMC] Insert Intel OCP 3.0 Card may cause Redfish and WEB UI can't get Processors information and DIMM Info.
3. [Redfish] Hitachi requirements is not ready.(Virtual Drive Information)

[Notice]:
1. For S5XQH, only support HW FAB4, FAB6 and FAB7.
2. For S5XQH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
3. For S5XQH, updating from 2.18 to 2.21, please use the socflash.
4. The password strength must be set at least 8 letters.
5. For S5XQH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
6. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
7. For S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
8. If upgrade BMC from 3.02.06 to 3.12.06, please follow below method:
	Method 1: follow below step:
	Step1: ipmitool raw 0x32 0x8f 0x01 0x02  
	Step2: ipmitool mc reset cold  
	Step2-1: Wait BMC Ready	
	Step3: ipmitool raw 0x32 0x8f 0x01 0x04  
	Step4: update 3.05 via webui or yafuflash
	If both fail, please use socflash for 3.05.
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10. RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.10.06
==========================================================================
Version: 3.10.06
Release Date: 2021.05.21
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.10.06_rom.ima with checksum          : 19BAB2A2
2. s5xhv3.10.06_rom.ima with MD5 checksum      : 30b69341327fcb088fb0237304f4fdd9
3. s5xhv3.10.06_rom.ima_enc with MD5 checksum  : 2bc581b9db436fbebb14baa6ebae5053

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R06_20210122 )
SKU 1~2	: R05 (S5X_2.5_R06_20210122 )
S5XQ:
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
S5XH/S5XQH:
1. [Redfish] HDS Redfish request: Server FRU(/redfish/v1/Chassis/Self/FRU)

[Bug Fixed]:
S5XH:
1. [BMC] Fix SMASH Functions.
2. [BMC] Set IPv6 static gateway address in BMC WEBUI, the address value is blank after login WEBUI again.
3. [BMC] Fix IERR dump function at CPU amount checking.
4. [BMC] Fix rkvm connect fail then webui also fail issue, BMC will stop user use rkvm when rkvm not ready.
5. [BMC] Fix BMC Image can't boot to the flashed image.
6. [BMC] Set IPv6 static gateway address in BMC WEBUI, the address value is blank after login WEBUI again.
7. [BMC] Fix fan duty will be set to 100% before BMC not ready while OCP card on board.
8. [BMC] Fix dashboard display issue on webui.
S5XQH:
1. [BMC] Fix full fan speed because wrong code judgement by pcie network card.  
2. [BMC] Remove pex polling task on other sku from all flash sku.

[Known Issue]:
1. [BMC] For S5XH, PSU LED and BP LED will be LID if insert Intel OCP 3.0 Card even is Power Off.
2. [BMC] Insert Intel OCP 3.0 Card may cause Redfish and WEB UI can't get Processors information and DIMM Info.
3. [Redfish] Hitachi requirements is not ready.(Virtual Drive Information)

[Notice]:
1. For S5X, only support HW FAB4, FAB6 and FAB7.
2. The password strength must be set at least 8 letters.
3. For S5X, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
4. For S5X and S5XQ, after updating 2.28, please use the BIOS 2A06 or later.
5. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
6. For S5X and S5XQ, after updating 3.01, please use the BIOS 3A04 or later.
7. If upgrade BMC from 3.02 to 3.07 or after, please follow below method:
8. If upgrade BMC from 3.02~ to 3.07 or after,
	Please follow below step:
	Step1: ipmitool raw 0x32 0x8f 0x01 0x02  
	Step2: ipmitool mc reset cold        
	Step2-1: Wait BMC Ready
	Step3: ipmitool raw 0x32 0x8f 0x01 0x04  
	Step4: update 3.07.06 or after via webui or yafuflash
	If fail, please use socflash for 3.07.06 or after 
9. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
10.RKVM(H5viewer) on webui might connect fail and then close the window within 5 minutes after AC on/BMC cold reset.
   Please wait for RKVM task reday 5 minute after AC on/BMC cold reset. Then user can use RKVM normally.
   If webui fail to open after RKVM(H5viewer) connection fail, please execute "BMC cold reset" and wait for more than 5 minutes. Then user can use RKVM normally.
   
==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.08.06
==========================================================================
Version: 3.08.06
Release Date: 2021.04.09
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.08.06_rom.ima with checksum          : 19B978C8
2. s5xhv3.08.06_rom.ima with MD5 checksum      : af7d4b76ddf3452829585025017d9a9b
3. s5xhv3.08.06_rom.ima_enc with MD5 checksum  : 166fca706d36b2e6d74899ce549a2375

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R05.0_20201110)
SKU 1~2	: R05 (S5X_2.5_R05.0_20201110)
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
S5XH:
1. Revert the LDAP fucntion from common submodule.
2. Fix the SEL parse about the sensor name of "OS".
3. Fix system could not power on when updating bios firmware.
4. Add SMASH Function Support.

[Bug Fixed]:
S5XH :
1. Fix when ac cycle, the conf would be broken.
2. Add the write disable/enable spi when ac cycle.
3. Fix WEB UI Sensor layout(The sensor value information is not fully shown)
4. Redfish Information missing.(Please use mallonex OCP Card)

[Known issue]:
1. PSU LED and BP LED will be LID if insert Intel OCP 3.0 Card even is Power Off.
2. [BMC] Radius function is not ready - Suport Windows Server Radius (NPS).
3. [Redfish] Hitachi requirements is not ready.
 (1)Server FRUs.
 (2)Virtual Drive Information. 
4. Insert Intel OCP 3.0 Card may cause Redfish and WEB UI can't get Processors information and DIMM Info.

[Notice]:
1. For S5X, only support HW FAB4, FAB6 and FAB7.
2. The password strength must be set at least 8 letters.
3. For S5X, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
4. For S5XQ, only support HW FAB6.
5. If upgrade BMC from 2.30 or before version to 3.00, please use the socflash to upgrade BMC.
6. For S5XH and S5XQH, after updating 3.02, please use the BIOS 3A04 or later.
7. If upgrade BMC from 3.02.06 to 3.08.06, please follow below method:
	Method 1: update 3.08.06 via webui or yafuflash twice continuously.
	Method 2: follow below step:
	Step1: ipmitool raw 0x32 0x8f 0x01 0x02  
	Step2: ipmitool mc reset cold        
	Step3: ipmitool raw 0x32 0x8f 0x01 0x04  
	Step3: update 3.08.06 via webui or yafuflash
	If both fail, please use socflash for 3.08.06
8. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.07.06
==========================================================================
Version: 3.07.06
Release Date: 2021.03.19
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.05
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.07.06_rom.ima with checksum          : 1B6FD0D4
2. s5xhv3.07.06_rom.ima with MD5 checksum      : 33b8d5a4a104720260ac1e5df3292580
3. s5xhv3.07.06_rom.ima_enc with MD5 checksum  : 61054c893811ac17a37114a218e089b8

[Fan Table]
Version:
S5X:
SKU 0	: R05 (S5X_3.5_R05.0_20201110)
SKU 1~2	: R05 (S5X_2.5_R05.0_20201110)
SKU 3~8	: R01 (S5XQ_QCT_2p5_FSC_Table_R01_20201221, S5XQ_QCT_3p5_FSC_Table_R01_20201221)

[Change/Add]:
1. [IPMI] Change to asynchronize for ipmb request
2. [IPMI] Fix the ME failed after DC cycle

[Bug Fixed]:
1. When using WebUI to update the BIOS firmware, the progress bar will go back to the middle after the Upgrade" is completed.
2. Add there should no AC lost event after DC off for 7 seconds flag definition.
3. Fix the HDD device present bounce bug.
4. Fix Pcie temp no reading at multi-card status.
5. The NVMe status doesn't need to change the 0xe2 channel.
6. Fix the nvme temperature and hdd status sensor sometimes show no reading.

[Known issue]:
1. PSU LED and BP LED will be LID if insert OCP 3.0 Card even is Power Off.
2. [BMC] Radius function is not ready - Suport Windows Server Radius (NPS).
3. [Redfish] Hitachi requirements is not ready.
 (1)Server FRUs.
 (2)Virtual Drive Information. 
4. Insert OCP 3.0 Card may cause Redfish and WEB UI can't get Processors information and DIMM Info.

[Notice]:
 1. For S5XH, only support HW FAB4, FAB6 and FAB7.
 2. The password strength must be set at least 8 letters.
 3. For S5XH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
 4. For S5XQ, only support HW FAB6.
 5. For S5XH and S5XQH, after updating 2.30, please use the BIOS 2A06 or later.
 6. For S5XH, if upgrade BMC from before version to 3.02, please use socflash tool to upgrade to v3.02.
 7. If upgrade BMC from 3.02~ to 3.07,
	Please follow below step:
	Step1: ipmitool raw 0x32 0x8f 0x01 0x02  
	Step2: ipmitool mc reset cold        
	Step3: ipmitool raw 0x32 0x8f 0x01 0x04  
	Step3: update 3.07.06 via webui or yafuflash
	If fail, please use socflash for 3.07.06
 8. BMC update via redfish will fail from the old version(~3.02) to new version(3.03~), 
    please use webui or yafuflash update at this case.
 9. For S5XH, after updating 3.01, please use the BIOS 3A04 or later. 	
 
==========================================================================
        S5XH series AST2500(A2) BMC FW Release v3.02.06
==========================================================================
Version: 3.02.06
Release Date: 2021.02.04
AMI Subversion Revision: AMI SPX RR12.3
Code Base: 3.00
DMTF Redfish Specification version: 1.8

[Utility]
1. Yafuflash (version 6.85.00)

[Prerequisite]
1. Please install the ipmitool.

[Firmware Images]:
1. s5xhv3.02.06_rom.ima with checksum          : 139BEEFA
2. s5xhv3.02.06_rom.ima with MD5 checksum      : afddaae384c74979843d9696b02a23c5
3. s5xhv3.02.06_rom.ima_enc with MD5 checksum  : 45685e864eb9bfe90088d5bdf0d6567e

[Fan Table]
Version:
S5XH:
SKU 0	: R5 (S5X_2.5_R05.0_20201110, S5X_3.5_R05.0_20201110)
SKU 1~2	: R5 (S5X_2.5_R05.0_20201110)
SKU 3~8	: R0 (S5XQ_FSC Table_R00_QCT_20200825_thermal)

[Change/Add]:
1. [RR12.3 AMI pure code update] Kernel update to 5.4 from 5.2 
2. Add Web BIOS Firmware update with preserve function. 
3. Redfish properties changed.
	[/redfish/v1/UpdateService/FirmwareInventory/CPLD]
		Add Version
	[/redfish/v1/UpdateService/FirmwareInventory/BIOS]
		Add Version
	[/redfish/v1/Chassis/Self/Power]
		Remove PowerControl-> PowerLimit
	[/redfish/v1/UpdateService]
		Add Oem->BIOS->BIOSPreserveNVRAM
		
[Bug Fixed]:
 1. [WEB]WEB UI can't update BMC.
 2. [REDFISH]In Redfish GET /Managers/Self Firmware version will show 2.30.xxxxx not 2.30.06 
 1. BMC watchdog reset after high inlet temperature to turn off system.
 2. BMC path Settings > System Firewall will change to Settings > Firewall after enter any page under it.
 3. [Web][FW upgrade] Fix CPLD firmware update.
 4. [WEB][Sensor Page] BMC sensor page will appear a lot of ""Chassis"" sensor at ""Discrete Sensor States"" section(Random 4/10).
 5. [WEB][Dashboard] The BMC version on WebUI menu bar is not matched with firmware package release note and IPMI mc info command.
 6. [WEB][Sensor Detail Page] Sensor detail page show multi record at sensor time line.
 7. [Bug] eTrack 349843 SSL certificate did not preserve after restore factory default with preserve all configuration fix again.
 8. Open Settings > IPMI Interfaces with Operator user privilege, WebUI will pup up error message and show incorrect IPMI Interfaces status.
 

[Known issue]:
1. [BMC]Can not read CPU/PCH temperature sometimes.  The fan speed will be Full duty when the CPU temperature disappears.
2. [BMC] Radius function is not ready - Suport Windows Server Radius (NPS).
3. [Redfish] Hitachi requirements is not ready.
 (1)Server FRUs.
 (2)Virtual Drive Information. 

[Notice]:
 1. For S5XH, only support HW FAB4, FAB6 and FAB7.
 2. For S5XH, before upgrading to v2.11, please use the MB-SKU-Tool to update the MB sku.
 3. For S5XH, updating from 2.18 to 2.21, please use the socflash.
 4. The password strength must be set at least 8 letters.
 5. For S5XH, FAB4 only support the 2KB size FP and FAB6 only support 16KB size FP.
 8. For S5XH, after updating 2.28, please use the BIOS 2A06 or later.
 9. If upgrade BMC from 2.30 or before version to 3.00 or after, please use the socflash to upgrade BMC.
10. For S5XH, after updating 3.01, please use the BIOS 3A04 or later. 

==========================================================================
        S5XH series AST2500(A2) BMC FW Release v2.30.06
==========================================================================
Version: 2.30.06
Release Date: 2020.12.31
Code Base: 2.11
DMTF Redfish Specification version: 1.8
AMI Subversion Revision: AMI SPX RR12.3

[Utility]
1. Yafuflash (version 6.78.0)

[Firmware Images]:
1. s5xhv2.30.06_rom.ima with checksum          : A4A259D2
2. s5xhv2.30.06_rom.ima with MD5 checksum      : e8ef1bc7b025d3b1329f30d39e1f3f82
3. s5xhv2.30.06_rom.ima_enc with MD5 checksum  : f2ea3b85c2f98552d3944c49062c1707

[Fan Table]
Version:
S5X:
SKU 0	: R5 (S5X_2.5_R05.0_20201110, S5X_3.5_R05.0_20201110)
SKU 1~2	: R5 (S5X_2.5_R05.0_20201110)
SKU 3~8	: R0 (S5XQ_FSC Table_R00_QCT_20200825_thermal)

[Change/Add]: 
N/A
[Bug Fixed]:
1. Severity or description of MCERR log within BMC SEL is ''Unspecified'' after trigger UPI Failover error by itp,
2. The FRU0 will become garbled text and cause FRU1/10 disappear after system do reboot. (ipmitool fru print)
3. MB FRU has garbage string. (Both of FP and NIC DRU are normal.)
4. The MB-FRU will disappear after system reboot. (DVT system, HW Rev: D2B Rework A / FP board: HW Rev: A1B)

[Known issue]:
1. The Fan_SYS_Status of SEL log on webUI will parse failed.
2. WEB UI can't update BMC. Please use Yafuflash to update BMC Firmware.
3. In Redfish GET /Managers/Self Firmware version will show 2.30.xxxxx not 2.30.06 
4. [Redfish] Hitachi requirements is not ready.
 (1).Server FRUs.
5. [BMC] Radius function is not ready - Suport Windows Server Radius (NPS).
	
[Notice]:
1. Only support HW FAB6 and FAB4.
2. The password strength must be set at least 8 letters.