AFU (AMI Firmware Update) is a package of utilities used 
to update the system BIOS under various operating systems.  

Note: AFU only works for APTIO with SMI FLASH support.
      Compatible with Aptio 5.

The package includes:

- AFULNX64 5.11.06.1854
- AFU User Guide

To run, extract all of the files from the folder with the name corresponding to the desired operating system.


Usage (applies to AFUWIN, AFUDOS, AFUEFI and AFUEFI64...
       for usage of AFUBSD and AFULNX see help files provided in their folders):
------------------------------------------------------------------
AFULNX_64 <BIOS ROM File Name> [Option 1] [Option 2]
Or
AFULNX_64 <Input or Output File Name> <Command>
Or
AFULNX_64 <Command>

BIOS ROM File Name
The mandatory field is used to specify path/filename of the BIOS ROM file with extension.

Commands
The mandatory field is used to select an operation mode.
- /FV             Copy Secure FV to EFI.
- /O		      Save current ROM image to file                            
- /U		      Display ROM File's ROMID                                  
- /S		      Refer to Options: /S                                      
- /D		      Verification test of given ROM File without flashing BIOS.
- /A:		      Refer to Options: /A:
- /OAD	      Refer to Options: /OAD
- /CLNEVNLOG      Clear Event Log.
Options
The optional field used to supply more information for flashing BIOS ROM. Following lists the supported optional parameters and format:
- /CMD: 	      Send special command to BIOS. /CMD:{xxx, xxx, xxx}
- /OEMCMD:	      Send special value to BIOS. /OEMCMD:xxx
- /DPC  	      Don't Check Aptio 4 and Aptio 5 platform.
- /PW:            Input password for file.
- /MEUL:          Program ME Entire Firmware Block, which supports
                  Production.BIN and PreProduction.BIN files.
- /Q  	      Silent execution                                          
- /X  	      Don't Check ROM ID                                        
- /S  	      Display current system's ROMID                            
- /JBC            Don't Check AC adapter and battery                     
- /CLRCFG 	      Program without preserving setup configuration
- /BCPALL 	      Save all question values before flash
- /HOLEOUT:       Save specific ROM Hole according to RomHole GUID.         
		      NewRomHole1.BIN /HOLEOUT:GUID                             
- /SP  	      Preserve Setup setting.                                   
- /Rn  	      Preserve SMBIOS type N during programming(n=0-255)        
- /R  	      Preserve ALL SMBIOS structure during programming          
- /B  	      Program Boot Block                                        
- /P  	      Program Main BIOS                                         
- /K  	      Program all non-critical blocks.
- /N  	      Program NVRAM                                             
- /Kn  	      Program n'th non-critical block(n=0-15). 
- /RLC:           To set default option for Rom layout change.(E:Entire ROM, A:
                  Abort, F:Force)
- /HOLE:  	      Update specific ROM Hole according to RomHole GUID.       
		      NewRomHole1.BIN /HOLE:GUID                                
- /L  	      Program all ROM Holes.                                    
- /Ln  	      Program n'th ROM Hole only(n=0-15).                       
- /ECUF  	      Update EC BIOS when newer version is detected.            
- /E  	      Program Embedded Controller Block.
- /ME 	      Program ME Entire Firmware Block.                   
- /MEUF           Program ME Ignition Firmware Block.
- /A: 	      Oem Activation file                                 
- /OAD  	      Delete Oem Activation key          
- /CLNEVNLOG      Clear Event Log.
- /CAPSULE  	Override Secure Flash policy to Capsule                   
- /RECOVERY  	Override Secure Flash policy to Recovery                  
- /EC  	      Program Embedded Controller Block. (Flash Type)           
- /REBOOT  	      Reboot after programming.                                 
- /SHUTDOWN       Shutdown after programming.                               
- /FDR		Flash Flash-Descriptor Region.(*1)
- /GBER		Flash GBE Region.(*1)
- /MER		Flash Entire ME Region.(*1)
- /OPR		Flash Operation Region of SPS.(*1)
- /PDR            Flash PDR Region.(*1)                                  

(*1)If BIOS ME Module have report, AFU will be show this command.

Rules
- Any parameter encolsed by < > is a mandatory field.
- Any parameter enclosed by [ ] is an optional field.
- <Commands> cannot co-exist with any [Options].
- Main BIOS image is default flashing area if no any option present.
- [/REBOOT], [/X], and [/S] will enable [/P] function automatically.
- If [/B] present alone, there is only the Boot Block area to be updated.
- If [/N] present alone, there is only the NVRAM area to be updated.
- If [/E] present alone, there is only the Embedded Controller block to be updated.
