=====================================================================
	Yafuflash utility Release version 6.86.28
=====================================================================
Utility:
1. Yafuflash (version 6.86.28)
   (for BMC RR12 LTE code base)

Supported BMC chip :  
1) AST2500


Before update firmware image please check as below:
please power off system before BIOS FW update 

[Notice]:
	AMI now not support Linux_x86_32 yafuflash, so we have already remove Linux_x86_32 folder
=====================================================================
	YAFUFlash Utility for BIOS Firmware update procedure
=====================================================================
[Notice]:
	in this directory
        Please fill in the <BIOS Image> with XXXX.BIN_enc file.
	1. Update BIOS FW via Out-of-Band command line:
		a) in Window, run "ubios_oob.bat <User name> <Password> <BMC IP> <BIOS Image>"
		   in Linux, run "./ubios_oob.sh <User name> <Password> <BMC IP> <BIOS Image>"
       
	2. Update BIOS FW with preserve nvram via Out-of-Band command line:
		a) in Window, run "ubios_preserve_nvram.bat <User name> <Password> <BMC IP> <BIOS Image>"
		   in Linux, run "./ubios_preserve_nvram.sh <User name> <Password> <BMC IP> <BIOS Image>"
